

[image: ]


	



Recommended PolyFerret® Sizes
Standard, Coupling, Abrasive & Grinding Projectiles
		
	PART NO.
	IMPERIAL
SIZE
	METRIC SIZE
(NOMINAL)
	APPROX. RECOMMENDED
PROJECTILE SIZE FOR NOZZLE



	HOSE
	I.D.
	I.D.
	HOSE WITHOUT COUPLINGS
	HOSE WITH COUPLINGS

	PNO6
	¼”
	6mm.
	S7 or S10
	C7

	PN08
	5/16”
	8mm.
	S12
	C10

	PN10
	3/8”
	10mm.
	S14
	C12

	PN13
	½”
	13mm.
	S18
	C16

	PN16
	5/8”
	16mm.
	S22
	C20

	PN19
	¾”
	19mm.
	S26
	C22

	PN25
	1”
	25mm.
	S33
	C33

	PN32
	1 ¼”
	32mm.
	S40
	C40

	PN38
	1 ½”
	38mm.
	S50
	C50

	PN50
	2”
	50mm.
	S60
	C60

	BSP
FITTINGS
	
	
	
	

	PNO6
	¼”
	6mm.
	
	C7

	PN10
	3/8”
	10mm.
	
	C12

	PN13
	½”
	13mm.
	
	C16

	PN16
	5/8”
	16mm.
	
	C20

	PN19
	¾”
	19mm.
	
	C22

	PN25
	1”
	25mm.
	
	C33

	PN32
	1 ¼”
	32mm.
	
	C40



	JIC FITTINGS AND TUBE
	
	
	JIC
	TUBE
A or S or C
	TUBE
GRINDING

	PNO6
	¼”
	6mm.
	C7
	A / S / C 7
	G7

	PN08
	5/16”
	8mm.
	C10
	A / S / C 10
	G10

	PN10
	3/8”
	10mm.
	C12
	A / S / C 12
	G10 / G12

	PN13
	½”
	13mm.
	C16
	A / S / C 16
	G14

	PN16
	5/8”
	16mm.
	C20
	A / S / C 20
	G16

	PN19
	¾”
	19mm.
	C22
	A / S / C 22
	G20

	PN25
	1”
	25mm.
	C33
	A / S / C 33
	G26

	PN32
	1 ¼”
	32mm.
	C40
	A / S / C 40
	G33

	PN38
	1 ½”
	38mm.
	C50
	A / S / C 50
	G40

	PN50
	2”
	50mm.
	C60
	A / S / C 60
	G50





Notes:  A = Abrasive  S = Standard  C = Coupling  G = Grinding.
These are minimum sizes. A larger size projectile may be used in some cases.
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